(footprint "PWM_module_ebay" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (attr smd)
  (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c8121568-d3f5-48c8-9ecf-a54c1a1074ad)
  )
  (fp_text value "PWM_module_ebay" (at 0 1 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp dd8648e9-e72b-41af-ac5a-778a58f169b2)
  )
  (fp_rect (start -2 -8.5) (end 31.5 8.5) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 544f39f6-64e8-4f0a-a78a-5e28b7872f5b))
  (pad "1" thru_hole roundrect (at 0 -1.27) (size 2.286 1.524) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25) (tstamp 6b50b86c-f9d8-4912-a87b-9d561db19997))
  (pad "2" thru_hole roundrect (at 0 1.27) (size 2.286 1.524) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25) (tstamp 5f68daa8-c144-4203-bee1-0e7dc9fd2d2a))
  (pad "3" thru_hole roundrect (at 27.94 -3.5) (size 2.286 1.524) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25) (tstamp 109eb1d6-b156-437a-a163-7bcc6259259e))
  (pad "4" thru_hole roundrect (at 27.94 0) (size 2.286 1.524) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25) (tstamp aae80b99-f5f7-4cee-b9d6-1e8589696882))
  (pad "5" thru_hole roundrect (at 27.94 3.5) (size 2.286 1.524) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25) (tstamp 39d93395-0259-4e7b-9e15-e09f030e816a))
)
