(footprint "Step-down_converter" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (attr smd)
  (fp_text reference "REF**" (at 1 -2 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 02961187-d897-402a-8be0-280efa86136e)
  )
  (fp_text value "Step-down_converter" (at 1 0 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 86ce3e0b-05da-49e1-bbdd-4b8a82d57320)
  )
  (fp_rect (start 9.398 -6.35) (end -8.382 5.334) (layer "F.SilkS") (width 0.12) (fill none) (tstamp a74d3364-cf5e-4ce8-81ee-30303d1a2fff))
  (fp_rect (start -8.382 -6.35) (end 9.398 5.334) (layer "F.CrtYd") (width 0.12) (fill none) (tstamp 2dc45bff-1695-4e57-9525-90c2d17683f1))
  (pad "IN+" thru_hole rect (at -7 4) (size 2 2) (drill 1) (layers *.Cu *.Mask) (tstamp f9cef32a-df9e-484b-9b98-5c39bed8e59f))
  (pad "IN-" thru_hole rect (at -7 -5) (size 2 2) (drill 1) (layers *.Cu *.Mask) (tstamp b207658a-2d2d-4567-aa6a-a6939ed82d9a))
  (pad "OUT+" thru_hole rect (at 8 4) (size 2 2) (drill 1) (layers *.Cu *.Mask) (tstamp 57a92d72-08d9-4070-ae87-6de89c192f43))
  (pad "OUT-" thru_hole rect (at 8 -5) (size 2 2) (drill 1) (layers *.Cu *.Mask) (tstamp b3710e17-dffb-4214-b6d9-79b3e34fd05c))
)
