(footprint "L298N Motor driver module-utan motorpads" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 09a028f6-0462-4b35-a49b-ef2c13c355bf)
  )
  (fp_text value "L298N Motor driver module-utan motorpads" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 14df8c27-1aca-4de8-bd30-28d03a31e6f6)
  )
  (fp_line (start -12.192 19.7) (end 9.398 19.7)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 317d2810-d3c2-49db-938a-bafe7f4e1e31))
  (fp_rect (start -21.7 -21.9) (end 21.7 21.9)
    (stroke (width 0.12) (type default)) (fill none) (layer "F.SilkS") (tstamp 5b17b7f5-435b-4a28-afb4-86ded0e884be))
  (pad "" np_thru_hole circle (at -18.5 -18.5) (size 3.5 3.5) (drill 3.5) (layers "F&B.Cu" "*.Mask") (tstamp c04b2057-c14b-4dd5-b142-15b98e9d5668))
  (pad "" np_thru_hole circle (at -18.5 18.5) (size 3.5 3.5) (drill 3.5) (layers "F&B.Cu" "*.Mask") (tstamp 7a2864d1-8946-4dc9-93a0-02a917a24fd8))
  (pad "" np_thru_hole circle (at 18.5 -18.5) (size 3.5 3.5) (drill 3.5) (layers "F&B.Cu" "*.Mask") (tstamp 269d31b6-76fe-44b5-8014-0153a125cf89))
  (pad "" np_thru_hole circle (at 18.5 18.5) (size 3.5 3.5) (drill 3.5) (layers "F&B.Cu" "*.Mask") (tstamp c86e2980-43bd-4dde-a031-8739fee66cba))
  (pad "1" thru_hole oval (at 2 19.7) (size 2 3) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 2a20db31-01a1-4353-ae5f-88685f485774))
  (pad "2" thru_hole oval (at 4.54 19.7) (size 2 3) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 00389037-846c-4418-9b22-7fd733ca52aa))
  (pad "3" thru_hole oval (at 7.08 19.7) (size 2 3) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 08d18f74-257d-41fb-b81c-4b1a4997e10a))
  (pad "4" thru_hole oval (at 9.62 19.7) (size 2 3) (drill 1) (layers "*.Cu" "*.Mask") (tstamp d53e5f93-12ba-4536-a4db-2ce58ccb8456))
  (pad "5" thru_hole oval (at 12.16 19.7) (size 2 3) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 6b708c4d-114c-4ca0-87da-43019ce568bd))
  (pad "6" thru_hole oval (at 14.7 19.7) (size 2 3) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 5d21a68b-46af-4933-ac21-2a94a7818f09))
  (pad "7" thru_hole oval (at -12.9 18.2) (size 4 7) (drill 1.2) (layers "*.Cu" "*.Mask") (tstamp 22dc6290-4fa9-4254-9657-42161eb64109))
  (pad "8" thru_hole oval (at -7.9 18.2) (size 4 7) (drill 1.2) (layers "*.Cu" "*.Mask") (tstamp fb5ddbfb-2f7d-4a7b-8c41-0e9c79aa84cc))
  (pad "9" thru_hole oval (at -2.9 18.2) (size 4 7) (drill 1.2) (layers "*.Cu" "*.Mask") (tstamp cdffeec5-53fa-4dc9-a305-b74eb46b6bfe))
)
