(footprint "PulseJack JB0011D01BNL"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "1 Port RJ45 Magjack Connector Through Hole 10/100 Base-T, AutoMDIX, https://www.amphenol-cs.com/media/wysiwyg/files/drawing/rjmg1bd3b8k1anr.pdf")
	(tags "RJ45 Magjack")
	(property "Reference" "REF**"
		(at -4.445 5.49 180)
		(layer "F.SilkS")
		(uuid "e2f1695c-beea-4fcf-8b80-b8ca5ba8d340")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "PulseJack JB0011D01BNL"
		(at -4.445 -18.23 180)
		(layer "F.Fab")
		(uuid "ba8f000b-59da-4929-ac44-88846ac40828")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "89d2aeb0-a4c7-4dcb-b7fc-8d84435efdde")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "eb6fea34-fdb8-4bf3-bc04-26e44275aa6a")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "70a2656a-bafa-4691-8d38-7c845d9a9789")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -12.42 -17.33)
		(end 3.53 -17.33)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "6cc8c013-9c97-410e-8b52-798376aa06f9")
	)
	(fp_line
		(start -12.42 -4.89)
		(end -12.42 -17.33)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "dfe51a95-bf40-4283-8584-c3bd5cc9df9e")
	)
	(fp_line
		(start -12.42 4.59)
		(end -12.42 -1.69)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "8246d8f2-1c6f-4b33-8d25-c618de02407e")
	)
	(fp_line
		(start 3.53 -17.33)
		(end 3.53 -4.89)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f47c6b12-f626-45aa-9068-5767b95e0936")
	)
	(fp_line
		(start 3.53 -1.69)
		(end 3.53 4.59)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0777e883-a211-4ec6-83de-d3a434fd515e")
	)
	(fp_line
		(start 3.53 4.59)
		(end -12.42 4.59)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "02396337-73e6-497a-8f0c-d054d6d0c6db")
	)
	(fp_line
		(start 3.73 1)
		(end 3.73 -1)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0c9cfb1c-8626-45ba-b8d0-0fa1d897dde5")
	)
	(fp_line
		(start -14.02 -4.04)
		(end -12.82 -5.24)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "13cdb4cc-fea5-44e3-93ef-ac453a62464a")
	)
	(fp_line
		(start -14.02 -2.54)
		(end -14.02 -4.04)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "a85fb57b-5bbf-4280-850d-8afa2455d39a")
	)
	(fp_line
		(start -12.82 -5.24)
		(end -12.82 -17.73)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "e2c5f1ff-8df1-4236-b76c-300e04f8790c")
	)
	(fp_line
		(start -12.82 -1.34)
		(end -14.02 -2.54)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "ce6674fd-2fbe-4f69-89a7-10eb73acbd10")
	)
	(fp_line
		(start -12.82 4.99)
		(end -12.82 -1.34)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "60a05c14-e1f9-4ada-a1af-593963ac1586")
	)
	(fp_line
		(start -12.82 4.99)
		(end 3.93 4.99)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "4fdd4f36-1a01-4604-96b0-b2181006ea98")
	)
	(fp_line
		(start 3.93 -17.73)
		(end -12.82 -17.73)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "bfd74dac-89ff-4170-b66a-da6e02ab8a10")
	)
	(fp_line
		(start 3.93 -5.24)
		(end 3.93 -17.73)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "a7ea8871-0814-496d-bea8-76acf87a9f1d")
	)
	(fp_line
		(start 3.93 -1.34)
		(end 5.13 -2.54)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "ce9b9799-5a6e-4d3c-ad71-51ecb5f3226b")
	)
	(fp_line
		(start 3.93 4.99)
		(end 3.93 -1.34)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "a7ea8871-0814-496d-bea8-76acf87a9f1d")
	)
	(fp_line
		(start 5.13 -4.04)
		(end 3.93 -5.24)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "35eb9022-e801-4ec2-b75e-575993ae22a7")
	)
	(fp_line
		(start 5.13 -2.54)
		(end 5.13 -4.04)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "42f37172-575a-4e35-ab04-4207d00c9215")
	)
	(fp_line
		(start -12.32 -17.23)
		(end 3.43 -17.23)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "3bcf90ed-72cf-43f6-9200-1af27dc71125")
	)
	(fp_line
		(start -12.32 4.49)
		(end -12.32 -17.23)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "0e51847c-5550-4434-a920-3207f3b327a4")
	)
	(fp_line
		(start 0 3.49)
		(end -1 4.49)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "2203cc90-7f47-4295-8157-870276d4dc86")
	)
	(fp_line
		(start 0 3.49)
		(end 1 4.49)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "aa2be614-88ae-4474-8f42-6dcd6743c3ee")
	)
	(fp_line
		(start 3.43 -17.23)
		(end 3.43 4.49)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "6433be6c-4de7-4dae-a169-d00a015d196a")
	)
	(fp_line
		(start 3.43 4.49)
		(end -12.32 4.49)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "98f93373-5da4-47b9-a4ca-c4dc9246ed79")
	)
	(fp_text user "${REFERENCE}"
		(at -4.445 -6.37 180)
		(layer "F.Fab")
		(uuid "9ca336cd-ca2e-4358-bf36-988a1e93b470")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "" np_thru_hole circle
		(at -10.16 -6.35 180)
		(size 3.25 3.25)
		(drill 3.25)
		(layers "F&B.Cu" "*.Mask")
		(uuid "f48b1e8e-4538-458d-a65c-3138e85ea983")
	)
	(pad "" np_thru_hole circle
		(at 1.27 -6.35 180)
		(size 3.25 3.25)
		(drill 3.25)
		(layers "F&B.Cu" "*.Mask")
		(uuid "185b9caa-e029-4e3c-ac0d-88faa14dbe70")
	)
	(pad "1" thru_hole rect
		(at 0 0 180)
		(size 1.9 1.9)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "e7b20907-2bab-4e95-a575-a415b5c81d21")
	)
	(pad "2" thru_hole circle
		(at -1.27 2.54 180)
		(size 1.9 1.9)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "795bd836-c6e1-4e60-8c0e-c390a64de36d")
	)
	(pad "3" thru_hole circle
		(at -2.54 0 180)
		(size 1.9 1.9)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "e8ffc943-c00a-44ac-890a-53d47631b4ca")
	)
	(pad "4" thru_hole circle
		(at -3.81 2.54 180)
		(size 1.9 1.9)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "07a28928-313b-4940-b033-f561fb74708a")
	)
	(pad "5" thru_hole circle
		(at -5.08 0 180)
		(size 1.9 1.9)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f45e2541-d577-4c9c-b663-888b4be2cd9d")
	)
	(pad "6" thru_hole circle
		(at -6.35 2.54 180)
		(size 1.9 1.9)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "c75da34c-c8bd-4693-b686-9e59682fd0df")
	)
	(pad "7" thru_hole circle
		(at -7.62 0 180)
		(size 1.9 1.9)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "d93d30c2-35fb-434c-a82d-d583066fc83d")
	)
	(pad "8" thru_hole circle
		(at -8.89 2.54 180)
		(size 1.9 1.9)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "df23d44a-7a80-4775-875f-744a84f07092")
	)
	(pad "9" thru_hole circle
		(at 1.8796 -11.2522 180)
		(size 1.89 1.89)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "31281c12-ca20-4a5f-84f9-96702a50100e")
	)
	(pad "10" thru_hole circle
		(at -0.6604 -9.7282 180)
		(size 1.89 1.89)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "1481ff80-5f30-4ef2-91da-ead74ebeaa80")
	)
	(pad "11" thru_hole circle
		(at -8.2296 -11.2522 180)
		(size 1.89 1.89)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "9804c560-faa5-4df3-9d54-539192cf2965")
	)
	(pad "12" thru_hole circle
		(at -10.7696 -9.7282 180)
		(size 1.89 1.89)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f7a2d297-559e-45fa-9e90-075150e8a9fa")
	)
	(pad "SH" thru_hole circle
		(at -12.319 -3.302 180)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "3a4032e9-a391-42a8-8d46-37a6a669af39")
	)
	(pad "SH" thru_hole circle
		(at 3.429 -3.302 180)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "9c410289-a5f6-43a2-b6d5-e00c7525c3d4")
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu" "F.SilkS")
		(uuid "8504694f-c10f-4788-9961-ef566cd97e6b")
		(name "No trace zone")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 3.683 -13.97) (xy -12.573 -13.97) (xy -12.573 -17.526) (xy 3.683 -17.526)
			)
		)
	)
	(model "${KICAD7_3DMODEL_DIR}/Connector_RJ.3dshapes/RJ45-01-J0011D01BNL.STEP"
		(hide yes)
		(offset
			(xyz -4.4 6.6 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 180)
		)
	)
	(model "../../../Utils/Kicad-utils/3d-Models/J0011D01BNL_3D.STEP"
		(offset
			(xyz -4.4 16.9 6.8)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 180)
		)
	)
)
