(footprint "4.0 TFT 480x320 led with sd and touch" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr through_hole)
  (fp_text reference "REF**" (at 6.858 -7.112 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 1dd33759-143b-476c-bb42-c5e5d445a2fc)
  )
  (fp_text value "4.0 TFT 480x320 led with sd and touch" (at 3.47 -0.254 90 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 1ce2bf2b-b61f-46da-a1cb-06e193ac5296)
  )
  (fp_rect (start -1.93 30.9) (end 106.07 -30.9)
    (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp 9717e78c-245e-4b0a-ba7e-ef5374b0c38c))
  (pad "" np_thru_hole circle (at 1.07 -27.5) (size 6 6) (drill 3.5) (layers "F&B.Cu" "*.Mask") (tstamp 7ce980db-52dc-41e1-bac4-30a0cf9df4f2))
  (pad "" np_thru_hole circle (at 1.07 27.5) (size 6 6) (drill 3.5) (layers "F&B.Cu" "*.Mask") (tstamp d2f64eb5-177b-453b-a52e-31c9cd53aa66))
  (pad "" np_thru_hole circle (at 103.07 -27.5) (size 6 6) (drill 3.5) (layers "F&B.Cu" "*.Mask") (tstamp 9edc280a-c2af-4851-92a3-2973bd93b7ea))
  (pad "" np_thru_hole circle (at 103.07 27.5) (size 6 6) (drill 3.5) (layers "F&B.Cu" "*.Mask") (tstamp f03fba2d-995e-47a0-b9be-5909be892403))
  (pad "1" thru_hole roundrect (at 104.14 3.81 180) (size 2.286 1.524) (drill 0.9) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25) (tstamp 21623806-8193-49aa-8e86-f5d741ee3217))
  (pad "2" thru_hole roundrect (at 104.14 1.27 180) (size 2.286 1.524) (drill 0.9) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25) (tstamp 1c8efd92-4e91-4579-bd5c-5fab3c9a7156))
  (pad "3" thru_hole roundrect (at 104.14 -1.27 180) (size 2.286 1.524) (drill 0.9) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25) (tstamp c0b8101a-448b-46a1-9a8a-2ff22c1b14db))
  (pad "4" thru_hole roundrect (at 104.14 -3.81 180) (size 2.286 1.524) (drill 0.9) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25) (tstamp a34698d6-085b-485a-ba4e-0184bb2cbfd8))
  (pad "5" thru_hole roundrect (at 0 16.51 180) (size 2.286 1.524) (drill 0.9) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25) (tstamp d099de14-88e2-441e-a73e-ff95baeb8e26))
  (pad "6" thru_hole roundrect (at 0 13.97 180) (size 2.286 1.524) (drill 0.9) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25) (tstamp 59a1ecf0-8d7b-4db7-8aa7-b858a90fc7be))
  (pad "7" thru_hole roundrect (at 0 11.43 180) (size 2.286 1.524) (drill 0.9) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25) (tstamp b96d741a-8459-4bdc-b8c3-996255ed9d94))
  (pad "8" thru_hole roundrect (at 0 8.89 180) (size 2.286 1.524) (drill 0.9) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25) (tstamp 378396b7-816f-412c-b398-2bfbec7f6a55))
  (pad "9" thru_hole roundrect (at 0 6.35 180) (size 2.286 1.524) (drill 0.9) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25) (tstamp 3f510b37-3d66-4b1f-a522-569a3c2d8bbf))
  (pad "10" thru_hole roundrect (at 0 3.81 180) (size 2.286 1.524) (drill 0.9) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25) (tstamp 434996e1-61bd-42ff-a716-8e2eded0b81d))
  (pad "11" thru_hole roundrect (at 0 1.27 180) (size 2.286 1.524) (drill 0.9) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25) (tstamp d04da8c4-1375-40f5-862d-89a40323615e))
  (pad "12" thru_hole roundrect (at 0 -1.27 180) (size 2.286 1.524) (drill 0.9) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25) (tstamp d3eb6fac-45c7-4fd1-9912-2d8c789ffa62))
  (pad "13" thru_hole roundrect (at 0 -3.81 180) (size 2.286 1.524) (drill 0.9) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25) (tstamp 925b72f2-8f72-452d-a630-3febc08cc9ad))
  (pad "14" thru_hole roundrect (at 0 -6.35 180) (size 2.286 1.524) (drill 0.9) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25) (tstamp b4fcf448-08be-496d-8886-fa111b5b3ed1))
  (pad "15" thru_hole roundrect (at 0 -8.89 180) (size 2.286 1.524) (drill 0.9) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25) (tstamp 71333f91-0375-4115-aff4-5c1287b2ffc3))
  (pad "16" thru_hole roundrect (at 0 -11.43 180) (size 2.286 1.524) (drill 0.9) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25) (tstamp 1da1d33c-0ecb-4e9c-810a-201946bf2333))
  (pad "17" thru_hole roundrect (at 0 -13.97 180) (size 2.286 1.524) (drill 0.9) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25) (tstamp da71bc08-e42f-44ea-865c-6032dc757532))
  (pad "18" thru_hole roundrect (at 0 -16.51 180) (size 2.286 1.524) (drill 0.9) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25) (tstamp e630b3ad-972b-48f8-8387-439339d1a82b))
)
