(footprint "USB_Micro-Hakan" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Micro USB AB receptable, right-angle inverted (https://www.molex.com/pdm_docs/sd/475900001_sd.pdf)")
  (tags "Micro AB USB SMD")
  (attr smd)
  (fp_text reference "REF**" (at 0 -4.8 -180) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 934339ec-1cb6-463e-8be7-53de8c8333c7)
  )
  (fp_text value "USB_Micro-Hakan" (at 0 3.5) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp cbe7cf3e-519b-4cc6-bb14-9eb244b4d642)
  )
  (fp_text user "PCB Edge" (at 0 1.45) (layer "Dwgs.User")
      (effects (font (size 0.4 0.4) (thickness 0.04)))
    (tstamp bab58309-66f6-4101-abc0-1146c4c6eb53)
  )
  (fp_text user "${REFERENCE}" (at 0 -1.5) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 9a98430f-5a6a-4beb-9df6-2ff5de8ad42d)
  )
  (fp_line (start -3.87 -3.27) (end -3.87 -1.2)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2d37630d-fc20-46e3-9f0a-37884fe92080))
  (fp_line (start -3.87 -3.27) (end -3 -3.27)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7a091366-bda5-4ae9-b8bb-05ca09dde226))
  (fp_line (start -3.87 1.2) (end -3.87 1.45)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0d46e52b-92f1-4829-89fc-4aaac518b86c))
  (fp_line (start 1 -3.8) (end 1.6 -3.8)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2da27fd0-40d0-4d12-8acb-9b0c4746f591))
  (fp_line (start 1.3 -3.5) (end 1 -3.8)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ec3cbbc1-7abb-4a2b-9614-d47a3494480c))
  (fp_line (start 1.3 -3.5) (end 1.6 -3.8)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 35601a70-353f-406d-bbd0-8caf92f19c0b))
  (fp_line (start 3 -3.27) (end 3.87 -3.27)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 40a7b295-350d-4143-baec-c6f8ff9d76d2))
  (fp_line (start 3.87 -3.27) (end 3.87 -1.2)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 74dfe2ea-e3fd-4caa-b764-c1de0b7a69ff))
  (fp_line (start 3.87 1.2) (end 3.87 1.45)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8ec0b9c7-7985-473b-bcc5-ddfb4408d2c9))
  (fp_line (start -3.75 1.45) (end -2.8 1.45)
    (stroke (width 0.1) (type solid)) (layer "Edge.Cuts") (tstamp 024d267c-18aa-4abd-a1d0-c92a6e485600))
  (fp_line (start -2.8 -0.125) (end -2.8 1.45)
    (stroke (width 0.1) (type solid)) (layer "Edge.Cuts") (tstamp 401e311c-0ca8-4584-8ff2-3f4f6b51d241))
  (fp_line (start -1.95 -0.125) (end -1.95 1.45)
    (stroke (width 0.1) (type solid)) (layer "Edge.Cuts") (tstamp 73d911a7-90a3-4d1d-a029-378744021085))
  (fp_line (start -1.95 1.45) (end 1.95 1.45)
    (stroke (width 0.1) (type solid)) (layer "Edge.Cuts") (tstamp ee5977e1-c184-40f7-a823-45eb668167aa))
  (fp_line (start 1.95 -0.125) (end 1.95 1.45)
    (stroke (width 0.1) (type solid)) (layer "Edge.Cuts") (tstamp 74b35cff-17e2-4b36-add6-6ec4112541a5))
  (fp_line (start 2.8 -0.125) (end 2.8 1.45)
    (stroke (width 0.1) (type solid)) (layer "Edge.Cuts") (tstamp 869611ae-d851-4622-abc5-aad71c6b09f1))
  (fp_line (start 2.8 1.45) (end 3.75 1.45)
    (stroke (width 0.1) (type solid)) (layer "Edge.Cuts") (tstamp 50bc56b1-3a29-4e1f-8652-d659f7d57da0))
  (fp_arc (start -2.8 -0.125) (mid -2.375 -0.55) (end -1.95 -0.125)
    (stroke (width 0.1) (type solid)) (layer "Edge.Cuts") (tstamp 7f5410bb-983e-4e57-b73a-0eb543c44190))
  (fp_arc (start 1.95 -0.125) (mid 2.375 -0.55) (end 2.8 -0.125)
    (stroke (width 0.1) (type solid)) (layer "Edge.Cuts") (tstamp 110f4d1a-d4c5-4e63-a5a9-f29f4fdc854e))
  (fp_line (start -5.18 -4.13) (end -5.18 2.65)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 002ef12b-00f9-48b1-a279-9f817643f514))
  (fp_line (start -5.18 -4.13) (end 5.18 -4.13)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5e020143-41e5-42c6-808c-eb743d1d2f89))
  (fp_line (start -5.18 2.65) (end 5.18 2.65)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0a5b36ae-286f-405c-9ec9-aabba86c2fd8))
  (fp_line (start 5.18 -4.13) (end 5.18 2.65)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7b6c0121-e313-40f8-9310-831434e7c888))
  (fp_line (start -3.75 -3.15) (end -3.75 1.45)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0fb604fc-b92e-45b6-8bda-e4899a9d5c8b))
  (fp_line (start -3.75 -3.15) (end 3.75 -3.15)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b12cf5c4-387b-4583-ac97-4f26bfd82512))
  (fp_line (start -3.75 1.45) (end 3.75 1.45)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 736ab801-951d-47eb-856b-bbd96669fe85))
  (fp_line (start -3.75 2.15) (end 3.75 2.15)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c70f2741-31b9-423c-a2a3-1fcfab4a62e2))
  (fp_line (start 3.75 -3.15) (end 3.75 1.45)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a10d755e-b990-4a0f-8473-2fa6c925a77c))
  (pad "" smd rect (at -3.5 0) (size 0.3 0.85) (layers "F.Paste") (tstamp f6d16555-361c-45c0-b638-e30497582a0c))
  (pad "" smd rect (at 3.5 0) (size 0.3 0.85) (layers "F.Paste") (tstamp 098f3983-cc81-4561-b6b3-5fbeddabea75))
  (pad "1" smd rect (at 1.3 -2.675) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp f18640f9-bb70-4637-8b80-13ef4e4668f7))
  (pad "2" smd rect (at 0.65 -2.675) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 14681c88-b094-46f2-ba05-0a108b5873e0))
  (pad "3" smd rect (at 0 -2.675) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp b99f8391-4192-462d-b63f-3c48dbc61c83))
  (pad "4" smd rect (at -0.65 -2.675) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 80b1b826-b2d9-4a3f-a60f-983859b1fe2d))
  (pad "5" smd rect (at -1.3 -2.675) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 7a5037d8-1adf-4802-9521-386cc4a58105))
  (pad "6" smd rect (at -3.7375 0) (size 0.875 1.9) (layers "F.Cu" "F.Mask") (tstamp 1e7c2782-72c9-4974-bc76-c1345656f1ec))
  (pad "6" smd rect (at 0 0) (size 2.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp bbaf77de-f7e5-4a41-9e1b-9dddcbff5b82))
  (pad "6" smd rect (at 3.7375 0) (size 0.875 1.9) (layers "F.Cu" "F.Mask") (tstamp b23bb249-4cd3-40fc-8105-d0d7b8908f58))
  (model "${KICAD6_3DMODEL_DIR}/Connector_USB.3dshapes/USB_Micro-AB_Molex_47590-0001.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
