
(footprint MODULE_ESP32_DEVKIT_V1 (layer F.Cu) (tedit 6381D09B)
  (descr "")
  (fp_text reference REF** (at -11.355 -27.36 0) (layer F.SilkS)
    (effects (font (size 1.0 1.0) (thickness 0.15)))
  )
  (fp_text value MODULE_ESP32_DEVKIT_V1 (at -0.56 27.36 0) (layer F.Fab)
    (effects (font (size 1.0 1.0) (thickness 0.15)))
  )
  (pad 1 thru_hole rect (at -12.7 -15.515) (size 2.0 2.0) (drill 1.02) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at -12.7 -12.975) (size 2.0 2.0) (drill 1.02) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at -12.7 -10.435) (size 2.0 2.0) (drill 1.02) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at -12.7 -7.895) (size 2.0 2.0) (drill 1.02) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at -12.7 -5.355) (size 2.0 2.0) (drill 1.02) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at -12.7 -2.815) (size 2.0 2.0) (drill 1.02) (layers *.Cu *.Mask))
  (pad 7 thru_hole circle (at -12.7 -0.275) (size 2.0 2.0) (drill 1.02) (layers *.Cu *.Mask))
  (pad 8 thru_hole circle (at -12.7 2.265) (size 2.0 2.0) (drill 1.02) (layers *.Cu *.Mask))
  (pad 9 thru_hole circle (at -12.7 4.805) (size 2.0 2.0) (drill 1.02) (layers *.Cu *.Mask))
  (pad 10 thru_hole circle (at -12.7 7.345) (size 2.0 2.0) (drill 1.02) (layers *.Cu *.Mask))
  (pad 11 thru_hole circle (at -12.7 9.885) (size 2.0 2.0) (drill 1.02) (layers *.Cu *.Mask))
  (pad 12 thru_hole circle (at -12.7 12.425) (size 2.0 2.0) (drill 1.02) (layers *.Cu *.Mask))
  (pad 13 thru_hole circle (at -12.7 14.965) (size 2.0 2.0) (drill 1.02) (layers *.Cu *.Mask))
  (pad 14 thru_hole circle (at -12.7 17.505) (size 2.0 2.0) (drill 1.02) (layers *.Cu *.Mask))
  (pad 15 thru_hole circle (at -12.7 20.045) (size 2.0 2.0) (drill 1.02) (layers *.Cu *.Mask))
  (pad 30 thru_hole circle (at 12.7 -15.515) (size 2.0 2.0) (drill 1.02) (layers *.Cu *.Mask))
  (pad 29 thru_hole circle (at 12.7 -12.975) (size 2.0 2.0) (drill 1.02) (layers *.Cu *.Mask))
  (pad 28 thru_hole circle (at 12.7 -10.435) (size 2.0 2.0) (drill 1.02) (layers *.Cu *.Mask))
  (pad 27 thru_hole circle (at 12.7 -7.895) (size 2.0 2.0) (drill 1.02) (layers *.Cu *.Mask))
  (pad 26 thru_hole circle (at 12.7 -5.355) (size 2.0 2.0) (drill 1.02) (layers *.Cu *.Mask))
  (pad 25 thru_hole circle (at 12.7 -2.815) (size 2.0 2.0) (drill 1.02) (layers *.Cu *.Mask))
  (pad 24 thru_hole circle (at 12.7 -0.275) (size 2.0 2.0) (drill 1.02) (layers *.Cu *.Mask))
  (pad 23 thru_hole circle (at 12.7 2.265) (size 2.0 2.0) (drill 1.02) (layers *.Cu *.Mask))
  (pad 22 thru_hole circle (at 12.7 4.805) (size 2.0 2.0) (drill 1.02) (layers *.Cu *.Mask))
  (pad 21 thru_hole circle (at 12.7 7.345) (size 2.0 2.0) (drill 1.02) (layers *.Cu *.Mask))
  (pad 20 thru_hole circle (at 12.7 9.885) (size 2.0 2.0) (drill 1.02) (layers *.Cu *.Mask))
  (pad 19 thru_hole circle (at 12.7 12.425) (size 2.0 2.0) (drill 1.02) (layers *.Cu *.Mask))
  (pad 18 thru_hole circle (at 12.7 14.965) (size 2.0 2.0) (drill 1.02) (layers *.Cu *.Mask))
  (pad 17 thru_hole circle (at 12.7 17.505) (size 2.0 2.0) (drill 1.02) (layers *.Cu *.Mask))
  (pad 16 thru_hole circle (at 12.7 20.045) (size 2.0 2.0) (drill 1.02) (layers *.Cu *.Mask))
  (pad None np_thru_hole circle (at -12.28 23.475) (size 3.0 3.0) (drill 3.0) (layers *.Cu *.Mask))
  (pad None np_thru_hole circle (at 12.23 23.475) (size 3.0 3.0) (drill 3.0) (layers *.Cu *.Mask))
  (pad None np_thru_hole circle (at 12.23 -23.475) (size 3.0 3.0) (drill 3.0) (layers *.Cu *.Mask))
  (pad None np_thru_hole circle (at -12.28 -23.475) (size 3.0 3.0) (drill 3.0) (layers *.Cu *.Mask))
  (fp_line (start -14.28 -25.475) (end -3.211 -25.475) (layer F.Fab) (width 0.127))
  (fp_line (start -3.211 -25.475) (end 3.5 -25.475) (layer F.Fab) (width 0.127))
  (fp_line (start 3.5 -25.475) (end 14.23 -25.475) (layer F.Fab) (width 0.127))
  (fp_line (start 14.23 -25.475) (end 14.23 25.475) (layer F.SilkS) (width 0.127))
  (fp_line (start 14.23 25.475) (end -14.28 25.475) (layer F.SilkS) (width 0.127))
  (fp_line (start -14.28 25.475) (end -14.28 -25.475) (layer F.Fab) (width 0.127))
  (fp_line (start -14.28 -25.475) (end 14.23 -25.475) (layer F.SilkS) (width 0.127))
  (fp_line (start -14.28 25.475) (end -14.28 -25.475) (layer F.SilkS) (width 0.127))
  (fp_circle (center -14.85 -15.515) (end -14.75 -15.515) (layer F.SilkS) (width 0.2))
  (fp_circle (center -14.85 -15.515) (end -14.75 -15.515) (layer F.Fab) (width 0.2))
  (fp_line (start 14.23 -25.475) (end 14.23 25.475) (layer F.Fab) (width 0.127))
  (fp_line (start -14.28 25.475) (end -8.91 25.475) (layer F.Fab) (width 0.127))
  (fp_line (start -8.91 25.475) (end 8.78 25.475) (layer F.Fab) (width 0.127))
  (fp_line (start 8.78 25.475) (end 14.23 25.475) (layer F.Fab) (width 0.127))
  (fp_line (start -8.91 25.475) (end -8.91 18.985) (layer F.Fab) (width 0.127))
  (fp_line (start -8.91 18.985) (end -8.91 6.355) (layer F.Fab) (width 0.127))
  (fp_line (start -8.91 6.355) (end 8.78 6.355) (layer F.Fab) (width 0.127))
  (fp_line (start 8.78 6.355) (end 8.78 18.985) (layer F.Fab) (width 0.127))
  (fp_line (start 8.78 18.985) (end 8.78 25.475) (layer F.Fab) (width 0.127))
  (fp_line (start -8.91 18.985) (end 8.78 18.985) (layer F.Fab) (width 0.127))
  (fp_line (start 3.5 -25.475) (end 3.5 -21.585) (layer F.Fab) (width 0.127))
  (fp_line (start 3.5 -21.585) (end -3.211 -21.585) (layer F.Fab) (width 0.127))
  (fp_line (start -3.211 -21.585) (end -3.211 -25.475) (layer F.Fab) (width 0.127))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.01)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -8.91 18.985)
        (xy 8.78 18.985)
        (xy 8.78 25.475)
        (xy -8.91 25.475)
      )
    )
  )
  (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.01)
    (keepout (tracks allowed) (vias not_allowed) (pads allowed ) (copperpour allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -8.91 18.985)
        (xy 8.78 18.985)
        (xy 8.78 25.475)
        (xy -8.91 25.475)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.01)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -8.91 18.985)
        (xy 8.78 18.985)
        (xy 8.78 25.475)
        (xy -8.91 25.475)
      )
    )
  )
  (fp_line (start -14.28 -25.475) (end -3.211 -25.475) (layer F.SilkS) (width 0.127))
  (fp_line (start -3.211 -25.475) (end 3.5 -25.475) (layer F.SilkS) (width 0.127))
  (fp_line (start 3.5 -25.475) (end 14.23 -25.475) (layer F.SilkS) (width 0.127))
  (fp_line (start -14.28 25.475) (end -14.28 -25.475) (layer F.SilkS) (width 0.127))
  (fp_line (start 14.23 -25.475) (end 14.23 25.475) (layer F.SilkS) (width 0.127))
  (fp_line (start -14.28 25.475) (end -8.91 25.475) (layer F.SilkS) (width 0.127))
  (fp_line (start -8.91 25.475) (end 8.78 25.475) (layer F.SilkS) (width 0.127))
  (fp_line (start 8.78 25.475) (end 14.23 25.475) (layer F.SilkS) (width 0.127))
  (fp_line (start -14.53 -25.725) (end -14.53 25.725) (layer F.CrtYd) (width 0.05))
  (fp_line (start -14.53 25.725) (end 14.48 25.725) (layer F.CrtYd) (width 0.05))
  (fp_line (start 14.48 25.725) (end 14.48 -25.725) (layer F.CrtYd) (width 0.05))
  (fp_line (start 14.48 -25.725) (end -14.53 -25.725) (layer F.CrtYd) (width 0.05))
)