(footprint "TCA_9548A_module" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a9653906-1f42-4915-a35e-72517899c891)
  )
  (fp_text value "TCA_9548A_module" (at 0 1 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp ff6d1b7e-1b2c-4d2a-931a-6d4d73547b13)
  )
  (fp_rect (start -10.16 -17.78) (end 12.7 15.24) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 7f03ab9f-5309-46c6-b1be-aa712f875925))
  (fp_rect (start -10.668 -18.288) (end 13.208 15.748) (layer "F.CrtYd") (width 0.12) (fill none) (tstamp 833d74bc-b858-4355-8236-3621ff0bed70))
  (pad "" np_thru_hole circle (at 1.27 -15.24) (size 5 5) (drill 3.2) (layers F&B.Cu *.Mask) (tstamp 1dac12bb-e465-4161-9224-558817b46c3a))
  (pad "" np_thru_hole circle (at 1.27 12.7) (size 5 5) (drill 3.2) (layers F&B.Cu *.Mask) (tstamp d9f6a103-7845-443a-955a-fd7a87994ee3))
  (pad "1" thru_hole rect (at -7.62 -15.24) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask) (tstamp 4ac03bfa-d64a-4788-b2a5-b070c780ab91))
  (pad "2" thru_hole roundrect (at -7.62 -12.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25) (tstamp dc981262-75db-4d92-af08-03d80404fd21))
  (pad "3" thru_hole roundrect (at -7.62 -10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25) (tstamp b3a63d9e-98fd-4df6-accc-60a5ff53ec03))
  (pad "4" thru_hole roundrect (at -7.62 -7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25) (tstamp 84fb0130-160c-4ea1-9fbd-21df04542f72))
  (pad "5" thru_hole roundrect (at -7.62 -5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25) (tstamp 6b46525f-9b03-4252-91ad-bd5bb1da540b))
  (pad "6" thru_hole roundrect (at -7.62 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25) (tstamp 902e11cb-0aba-4bfd-8498-db20a1300fb2))
  (pad "7" thru_hole roundrect (at -7.62 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25) (tstamp 4ac83c5e-cd3c-45d0-9b2b-2352c7cc7bbb))
  (pad "8" thru_hole roundrect (at -7.62 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25) (tstamp c41cbd59-e088-4cb9-abf5-0f2ece40d145))
  (pad "9" thru_hole roundrect (at -7.62 5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25) (tstamp 838a8ff9-57e5-4d8f-9074-564dbdcb1e60))
  (pad "10" thru_hole roundrect (at -7.62 7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25) (tstamp c262cfc5-31e3-444a-aec4-8a6e79b57c0d))
  (pad "11" thru_hole roundrect (at -7.62 10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25) (tstamp e03aa8f9-49e8-4331-9ae0-c600d010a7d0))
  (pad "12" thru_hole roundrect (at -7.62 12.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25) (tstamp e048d497-97c9-424b-b599-3cb2dd14dc82))
  (pad "13" thru_hole roundrect (at 10.16 12.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25) (tstamp 48e6fec1-2792-457f-9d81-2980b94f33bd))
  (pad "14" thru_hole roundrect (at 10.16 10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25) (tstamp 71041c6e-ef70-4e01-90b1-876593a19699))
  (pad "15" thru_hole roundrect (at 10.16 7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25) (tstamp dd299121-d1fc-45c2-9757-c34a748f5f5a))
  (pad "16" thru_hole roundrect (at 10.16 5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25) (tstamp 13a0a00f-bf02-49b6-9651-f1124311b2dc))
  (pad "17" thru_hole roundrect (at 10.16 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25) (tstamp 600d6432-936e-444c-981a-00e5908475ae))
  (pad "18" thru_hole roundrect (at 10.16 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25) (tstamp cf975e27-2002-4acb-acfb-c5ceeee2ab70))
  (pad "19" thru_hole roundrect (at 10.16 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25) (tstamp 32867613-7e95-40e0-a5e2-fdec80342970))
  (pad "20" thru_hole roundrect (at 10.16 -5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25) (tstamp 7aadf216-889b-49f9-9450-f3202ed6213b))
  (pad "21" thru_hole roundrect (at 10.16 -7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25) (tstamp 8dc3033e-c4c1-48b9-8ce5-522f131bdf3d))
  (pad "22" thru_hole roundrect (at 10.16 -10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25) (tstamp 598aba67-4064-4582-940b-15dc2358a70c))
  (pad "23" thru_hole roundrect (at 10.16 -12.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25) (tstamp d394e805-e59f-4704-bcc0-fd7e52a23959))
  (pad "24" thru_hole roundrect (at 10.16 -15.24) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25) (tstamp c83cae79-a3e6-46dd-83e7-fe9b6c86a3f1))
)
