(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "LAN9252_PT" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -60.96 59.69 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Value" "LAN9252_PT" (at -29.21 -60.96 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Footprint" "LAN9252_PT:QFP50P1200X1200X120-65N" (at -5.08 6.35 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Datasheet" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "MF" "Microchip" (at -1.27 -13.97 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MAXIMUM_PACKAGE_HEIGHT" "1.2 mm" (at 0 -2.54 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Package" "TQFP-64 Microchip" (at -1.27 -11.43 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Price" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Check_prices" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "STANDARD" "IPC 7351B" (at -1.27 -5.08 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "PARTREV" "04-08-15" (at -1.27 -13.97 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "SnapEDA_Link" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MP" "LAN9252/PT" (at -2.54 3.81 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Purchase-URL" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Description" "\nEthernet Controller 10/100 Base-FX/T/TX PHY SPI Interface 64-TQFP-EP (10x10)\n" (at -1.27 10.16 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Availability" "" (at 0 -2.54 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MANUFACTURER" "Microchip Technology" (at -1.27 -8.89 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (symbol "LAN9252_PT_0_0"
      (rectangle (start -29.21 58.42) (end 60.96 -59.69)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input line (at -34.29 -2.54 0) (length 5.08)
        (name "OSCI" (effects (font (size 1.016 1.016))))
        (number "1" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -34.29 12.7 0) (length 5.08)
        (name "FXSDB/FXLOSB/~{FXSDENB}" (effects (font (size 1.016 1.016))))
        (number "10" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -34.29 30.48 0) (length 5.08)
        (name "~{RST}" (effects (font (size 1.016 1.016))))
        (number "11" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 66.04 -10.16 180) (length 5.08)
        (name "D2/AD2/SOF/SIO2" (effects (font (size 1.016 1.016))))
        (number "12" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 66.04 -7.62 180) (length 5.08)
        (name "D1/AD1/EOF/SO/SIO1" (effects (font (size 1.016 1.016))))
        (number "13" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 66.04 59.69 180) (length 5.08)
        (name "VDDIO" (effects (font (size 1.016 1.016))))
        (number "14" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 66.04 -40.64 180) (length 5.08)
        (name "D14/AD14/DIGIO8/GPI8/GPO8/MII_TXD3/~{TX_SHIFT1}" (effects (font (size 1.016 1.016))))
        (number "15" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 66.04 -38.1 180) (length 5.08)
        (name "D13/AD13/DIGIO7/GPI7/GPO7/MII_TXD2/~{TX_SHIFT0}" (effects (font (size 1.016 1.016))))
        (number "16" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 66.04 -5.08 180) (length 5.08)
        (name "D0/AD0/WD_STATE/SI/SIO0" (effects (font (size 1.016 1.016))))
        (number "17" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -34.29 -25.4 0) (length 5.08)
        (name "SYNC1/LATCH1" (effects (font (size 1.016 1.016))))
        (number "18" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 66.04 -27.94 180) (length 5.08)
        (name "D9/AD9/LATCH_IN/SCK" (effects (font (size 1.016 1.016))))
        (number "19" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at -34.29 -5.08 0) (length 5.08)
        (name "OSCO" (effects (font (size 1.016 1.016))))
        (number "2" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 66.04 60.96 180) (length 5.08)
        (name "VDDIO" (effects (font (size 1.016 1.016))))
        (number "20" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 66.04 -35.56 180) (length 5.08)
        (name "D12/AD12/DIGIO6/GPI6/GPO6/MII_TXD1" (effects (font (size 1.016 1.016))))
        (number "21" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 66.04 -33.02 180) (length 5.08)
        (name "D11/AD11/DIGIO5/GPI5/GPO5/MII_TXD0" (effects (font (size 1.016 1.016))))
        (number "22" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 66.04 -30.48 180) (length 5.08)
        (name "D10/AD10/DIGIO4/GPI4/GPO4/MII_TXEN" (effects (font (size 1.016 1.016))))
        (number "23" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 66.04 55.88 180) (length 5.08)
        (name "VDDCR" (effects (font (size 1.016 1.016))))
        (number "24" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -34.29 -35.56 0) (length 5.08)
        (name "A1/ALELO/OE_EXT/MII_CLK25" (effects (font (size 1.016 1.016))))
        (number "25" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -34.29 -40.64 0) (length 5.08)
        (name "A3/DIGIO11/GPI11/GPO11/MII_RXDV" (effects (font (size 1.016 1.016))))
        (number "26" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -34.29 -43.18 0) (length 5.08)
        (name "A4/DIGIO12/GPI12/GPO12/MII_RXD0" (effects (font (size 1.016 1.016))))
        (number "27" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -34.29 -30.48 0) (length 5.08)
        (name "CS/DIGIO13/GPI13/GPO13/MII_RXD1" (effects (font (size 1.016 1.016))))
        (number "28" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -34.29 -38.1 0) (length 5.08)
        (name "A2/ALEHI/DIGIO10/GPI10/GPO10/LINKACTLED2/~{MII_LINKPOL}" (effects (font (size 1.016 1.016))))
        (number "29" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 66.04 48.26 180) (length 5.08)
        (name "OSCVDD12" (effects (font (size 1.016 1.016))))
        (number "3" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 66.04 2.54 180) (length 5.08)
        (name "WR/ENB/DIGIO14/GPI14/GPO14/MII_RXD2" (effects (font (size 1.016 1.016))))
        (number "30" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 66.04 0 180) (length 5.08)
        (name "RD/RD_WR/DIGIO15/GPI15/GPO15/MII_RXD3" (effects (font (size 1.016 1.016))))
        (number "31" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 66.04 62.23 180) (length 5.08)
        (name "VDDIO" (effects (font (size 1.016 1.016))))
        (number "32" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 66.04 -43.18 180) (length 5.08)
        (name "A0/D15/AD15/DIGIO9/GPI9/GPO9/MII_RXER" (effects (font (size 1.016 1.016))))
        (number "33" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -34.29 -22.86 0) (length 5.08)
        (name "SYNC0/LATCH0" (effects (font (size 1.016 1.016))))
        (number "34" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 66.04 -12.7 180) (length 5.08)
        (name "D3/AD3/WD_TRIG/SIO3" (effects (font (size 1.016 1.016))))
        (number "35" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 66.04 -20.32 180) (length 5.08)
        (name "D6/AD6/DIGIO0/GPI0/GPO0/MII_RXCLK" (effects (font (size 1.016 1.016))))
        (number "36" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 66.04 63.5 180) (length 5.08)
        (name "VDDIO" (effects (font (size 1.016 1.016))))
        (number "37" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 66.04 54.61 180) (length 5.08)
        (name "VDDCR" (effects (font (size 1.016 1.016))))
        (number "38" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 66.04 -22.86 180) (length 5.08)
        (name "D7/AD7/DIGIO1/GPI1/GPO1/MII_MDC" (effects (font (size 1.016 1.016))))
        (number "39" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 66.04 -55.88 180) (length 5.08)
        (name "OSCVSS" (effects (font (size 1.016 1.016))))
        (number "4" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 66.04 -25.4 180) (length 5.08)
        (name "D8/AD8/DIGIO2/GPI2/GPO2/MII_MDIO" (effects (font (size 1.016 1.016))))
        (number "40" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at 66.04 -48.26 180) (length 5.08)
        (name "TESTMODE" (effects (font (size 1.016 1.016))))
        (number "41" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -34.29 5.08 0) (length 5.08)
        (name "EESDA/TMS" (effects (font (size 1.016 1.016))))
        (number "42" (effects (font (size 1.016 1.016))))
      )
      (pin output clock (at -34.29 2.54 0) (length 5.08)
        (name "EESCL/TCK" (effects (font (size 1.016 1.016))))
        (number "43" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at 66.04 30.48 180) (length 5.08)
        (name "IRQ" (effects (font (size 1.016 1.016))))
        (number "44" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -34.29 -17.78 0) (length 5.08)
        (name "RUNLED/~{E2PSIZE}" (effects (font (size 1.016 1.016))))
        (number "45" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -34.29 -12.7 0) (length 5.08)
        (name "LINKACTLED1/TDI/~{CHIP_MODE1}" (effects (font (size 1.016 1.016))))
        (number "46" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 66.04 58.42 180) (length 5.08)
        (name "VDDIO" (effects (font (size 1.016 1.016))))
        (number "47" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at -34.29 -10.16 0) (length 5.08)
        (name "LINKACTLED0/TDO/~{CHIP_MODE0}" (effects (font (size 1.016 1.016))))
        (number "48" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 66.04 -15.24 180) (length 5.08)
        (name "D4/AD4/DIGIO3/GPI3/GPO3/MII_LINK" (effects (font (size 1.016 1.016))))
        (number "49" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 66.04 50.8 180) (length 5.08)
        (name "VDD33" (effects (font (size 1.016 1.016))))
        (number "5" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 66.04 -17.78 180) (length 5.08)
        (name "D5/AD5/OUTVALID/SCS#" (effects (font (size 1.016 1.016))))
        (number "50" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 66.04 38.1 180) (length 5.08)
        (name "VDD33TXRX1" (effects (font (size 1.016 1.016))))
        (number "51" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 66.04 22.86 180) (length 5.08)
        (name "TXNA" (effects (font (size 1.016 1.016))))
        (number "52" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 66.04 25.4 180) (length 5.08)
        (name "TXPA" (effects (font (size 1.016 1.016))))
        (number "53" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 66.04 17.78 180) (length 5.08)
        (name "RXNA" (effects (font (size 1.016 1.016))))
        (number "54" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 66.04 20.32 180) (length 5.08)
        (name "RXPA" (effects (font (size 1.016 1.016))))
        (number "55" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 66.04 45.72 180) (length 5.08)
        (name "VDD12TX1" (effects (font (size 1.016 1.016))))
        (number "56" (effects (font (size 1.016 1.016))))
      )
      (pin passive line (at -34.29 -48.26 0) (length 5.08)
        (name "RBIAS" (effects (font (size 1.016 1.016))))
        (number "57" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 66.04 40.64 180) (length 5.08)
        (name "VDD33BIAS" (effects (font (size 1.016 1.016))))
        (number "58" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 66.04 43.18 180) (length 5.08)
        (name "VDD12TX2" (effects (font (size 1.016 1.016))))
        (number "59" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 66.04 53.34 180) (length 5.08)
        (name "VDDCR" (effects (font (size 1.016 1.016))))
        (number "6" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 66.04 10.16 180) (length 5.08)
        (name "RXPB" (effects (font (size 1.016 1.016))))
        (number "60" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 66.04 7.62 180) (length 5.08)
        (name "RXNB" (effects (font (size 1.016 1.016))))
        (number "61" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 66.04 15.24 180) (length 5.08)
        (name "TXPB" (effects (font (size 1.016 1.016))))
        (number "62" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 66.04 12.7 180) (length 5.08)
        (name "TXNB" (effects (font (size 1.016 1.016))))
        (number "63" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 66.04 35.56 180) (length 5.08)
        (name "VDD33TXRX2" (effects (font (size 1.016 1.016))))
        (number "64" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 66.04 -53.34 180) (length 5.08)
        (name "VSS" (effects (font (size 1.016 1.016))))
        (number "65" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -34.29 25.4 0) (length 5.08)
        (name "REG_EN" (effects (font (size 1.016 1.016))))
        (number "7" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -34.29 17.78 0) (length 5.08)
        (name "~{FXLOSEN}" (effects (font (size 1.016 1.016))))
        (number "8" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -34.29 15.24 0) (length 5.08)
        (name "FXSDA/FXLOSA/~{FXSDENA}" (effects (font (size 1.016 1.016))))
        (number "9" (effects (font (size 1.016 1.016))))
      )
    )
  )
)
