# Channel table for Poço Redondo - SE - Brazil
# Source: https://portalbsd.com.br/terrestres_channels.php?cidade=2327

# Physical channel 17 (virtual 17.2)
[TVC SE, TV Liberdade]
	DELIVERY_SYSTEM = ISDBT
	BANDWIDTH_HZ = 6000000
	FREQUENCY = 491142857
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	ISDBT_LAYER_ENABLED = 7
	ISDBT_SOUND_BROADCASTING = 0
	ISDBT_SB_SUBCHANNEL_ID = 0
	ISDBT_SB_SEGMENT_IDX = 0
	ISDBT_SB_SEGMENT_COUNT = 0
	ISDBT_LAYERA_FEC = AUTO
	ISDBT_LAYERA_MODULATION = QAM/AUTO
	ISDBT_LAYERA_SEGMENT_COUNT = 0
	ISDBT_LAYERA_TIME_INTERLEAVING = 0
	ISDBT_LAYERB_FEC = AUTO
	ISDBT_LAYERB_MODULATION = QAM/AUTO
	ISDBT_LAYERB_SEGMENT_COUNT = 0
	ISDBT_LAYERB_TIME_INTERLEAVING = 0
	ISDBT_LAYERC_FEC = AUTO
	ISDBT_LAYERC_MODULATION = QAM/AUTO
	ISDBT_LAYERC_SEGMENT_COUNT = 0
	ISDBT_LAYERC_TIME_INTERLEAVING = 0

# Physical channel 19 (virtual 19.2)
[Rede SÃ©culo 21, Rede SÃ©culo 21 Educa]
	DELIVERY_SYSTEM = ISDBT
	BANDWIDTH_HZ = 6000000
	FREQUENCY = 503142857
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	ISDBT_LAYER_ENABLED = 7
	ISDBT_SOUND_BROADCASTING = 0
	ISDBT_SB_SUBCHANNEL_ID = 0
	ISDBT_SB_SEGMENT_IDX = 0
	ISDBT_SB_SEGMENT_COUNT = 0
	ISDBT_LAYERA_FEC = AUTO
	ISDBT_LAYERA_MODULATION = QAM/AUTO
	ISDBT_LAYERA_SEGMENT_COUNT = 0
	ISDBT_LAYERA_TIME_INTERLEAVING = 0
	ISDBT_LAYERB_FEC = AUTO
	ISDBT_LAYERB_MODULATION = QAM/AUTO
	ISDBT_LAYERB_SEGMENT_COUNT = 0
	ISDBT_LAYERB_TIME_INTERLEAVING = 0
	ISDBT_LAYERC_FEC = AUTO
	ISDBT_LAYERC_MODULATION = QAM/AUTO
	ISDBT_LAYERC_SEGMENT_COUNT = 0
	ISDBT_LAYERC_TIME_INTERLEAVING = 0

# Physical channel 26 (virtual 40.1)
[TV Sul Bahia]
	DELIVERY_SYSTEM = ISDBT
	BANDWIDTH_HZ = 6000000
	FREQUENCY = 545142857
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	ISDBT_LAYER_ENABLED = 7
	ISDBT_SOUND_BROADCASTING = 0
	ISDBT_SB_SUBCHANNEL_ID = 0
	ISDBT_SB_SEGMENT_IDX = 0
	ISDBT_SB_SEGMENT_COUNT = 0
	ISDBT_LAYERA_FEC = AUTO
	ISDBT_LAYERA_MODULATION = QAM/AUTO
	ISDBT_LAYERA_SEGMENT_COUNT = 0
	ISDBT_LAYERA_TIME_INTERLEAVING = 0
	ISDBT_LAYERB_FEC = AUTO
	ISDBT_LAYERB_MODULATION = QAM/AUTO
	ISDBT_LAYERB_SEGMENT_COUNT = 0
	ISDBT_LAYERB_TIME_INTERLEAVING = 0
	ISDBT_LAYERC_FEC = AUTO
	ISDBT_LAYERC_MODULATION = QAM/AUTO
	ISDBT_LAYERC_SEGMENT_COUNT = 0
	ISDBT_LAYERC_TIME_INTERLEAVING = 0

# Physical channel 31 (virtual 2.4)
[TV Brasil, Canal Gov, Canal EducaÃ§Ã£o, Canal SaÃºde]
	DELIVERY_SYSTEM = ISDBT
	BANDWIDTH_HZ = 6000000
	FREQUENCY = 575142857
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	ISDBT_LAYER_ENABLED = 7
	ISDBT_SOUND_BROADCASTING = 0
	ISDBT_SB_SUBCHANNEL_ID = 0
	ISDBT_SB_SEGMENT_IDX = 0
	ISDBT_SB_SEGMENT_COUNT = 0
	ISDBT_LAYERA_FEC = AUTO
	ISDBT_LAYERA_MODULATION = QAM/AUTO
	ISDBT_LAYERA_SEGMENT_COUNT = 0
	ISDBT_LAYERA_TIME_INTERLEAVING = 0
	ISDBT_LAYERB_FEC = AUTO
	ISDBT_LAYERB_MODULATION = QAM/AUTO
	ISDBT_LAYERB_SEGMENT_COUNT = 0
	ISDBT_LAYERB_TIME_INTERLEAVING = 0
	ISDBT_LAYERC_FEC = AUTO
	ISDBT_LAYERC_MODULATION = QAM/AUTO
	ISDBT_LAYERC_SEGMENT_COUNT = 0
	ISDBT_LAYERC_TIME_INTERLEAVING = 0

# Physical channel 32 (virtual 9.1)
[TV Sergipe]
	DELIVERY_SYSTEM = ISDBT
	BANDWIDTH_HZ = 6000000
	FREQUENCY = 581142857
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	ISDBT_LAYER_ENABLED = 7
	ISDBT_SOUND_BROADCASTING = 0
	ISDBT_SB_SUBCHANNEL_ID = 0
	ISDBT_SB_SEGMENT_IDX = 0
	ISDBT_SB_SEGMENT_COUNT = 0
	ISDBT_LAYERA_FEC = AUTO
	ISDBT_LAYERA_MODULATION = QAM/AUTO
	ISDBT_LAYERA_SEGMENT_COUNT = 0
	ISDBT_LAYERA_TIME_INTERLEAVING = 0
	ISDBT_LAYERB_FEC = AUTO
	ISDBT_LAYERB_MODULATION = QAM/AUTO
	ISDBT_LAYERB_SEGMENT_COUNT = 0
	ISDBT_LAYERB_TIME_INTERLEAVING = 0
	ISDBT_LAYERC_FEC = AUTO
	ISDBT_LAYERC_MODULATION = QAM/AUTO
	ISDBT_LAYERC_SEGMENT_COUNT = 0
	ISDBT_LAYERC_TIME_INTERLEAVING = 0

# Physical channel 36 (virtual 10.4)
[TV CÃ¢mara, TV Senado, RÃ¡dio CÃ¢mara]
	DELIVERY_SYSTEM = ISDBT
	BANDWIDTH_HZ = 6000000
	FREQUENCY = 605142857
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	ISDBT_LAYER_ENABLED = 7
	ISDBT_SOUND_BROADCASTING = 0
	ISDBT_SB_SUBCHANNEL_ID = 0
	ISDBT_SB_SEGMENT_IDX = 0
	ISDBT_SB_SEGMENT_COUNT = 0
	ISDBT_LAYERA_FEC = AUTO
	ISDBT_LAYERA_MODULATION = QAM/AUTO
	ISDBT_LAYERA_SEGMENT_COUNT = 0
	ISDBT_LAYERA_TIME_INTERLEAVING = 0
	ISDBT_LAYERB_FEC = AUTO
	ISDBT_LAYERB_MODULATION = QAM/AUTO
	ISDBT_LAYERB_SEGMENT_COUNT = 0
	ISDBT_LAYERB_TIME_INTERLEAVING = 0
	ISDBT_LAYERC_FEC = AUTO
	ISDBT_LAYERC_MODULATION = QAM/AUTO
	ISDBT_LAYERC_SEGMENT_COUNT = 0
	ISDBT_LAYERC_TIME_INTERLEAVING = 0

# Physical channel 43 (virtual 43.1)
[TV Atalaia]
	DELIVERY_SYSTEM = ISDBT
	BANDWIDTH_HZ = 6000000
	FREQUENCY = 647142857
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	ISDBT_LAYER_ENABLED = 7
	ISDBT_SOUND_BROADCASTING = 0
	ISDBT_SB_SUBCHANNEL_ID = 0
	ISDBT_SB_SEGMENT_IDX = 0
	ISDBT_SB_SEGMENT_COUNT = 0
	ISDBT_LAYERA_FEC = AUTO
	ISDBT_LAYERA_MODULATION = QAM/AUTO
	ISDBT_LAYERA_SEGMENT_COUNT = 0
	ISDBT_LAYERA_TIME_INTERLEAVING = 0
	ISDBT_LAYERB_FEC = AUTO
	ISDBT_LAYERB_MODULATION = QAM/AUTO
	ISDBT_LAYERB_SEGMENT_COUNT = 0
	ISDBT_LAYERB_TIME_INTERLEAVING = 0
	ISDBT_LAYERC_FEC = AUTO
	ISDBT_LAYERC_MODULATION = QAM/AUTO
	ISDBT_LAYERC_SEGMENT_COUNT = 0
	ISDBT_LAYERC_TIME_INTERLEAVING = 0

