# Channel table for Santo Antônio De Goiás - GO - Brazil
# Source: https://portalbsd.com.br/terrestres_channels.php?cidade=3548

# Physical channel 15 (virtual 15.1)
[TV UFG]
	DELIVERY_SYSTEM = ISDBT
	BANDWIDTH_HZ = 6000000
	FREQUENCY = 479142857
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	ISDBT_LAYER_ENABLED = 7
	ISDBT_SOUND_BROADCASTING = 0
	ISDBT_SB_SUBCHANNEL_ID = 0
	ISDBT_SB_SEGMENT_IDX = 0
	ISDBT_SB_SEGMENT_COUNT = 0
	ISDBT_LAYERA_FEC = AUTO
	ISDBT_LAYERA_MODULATION = QAM/AUTO
	ISDBT_LAYERA_SEGMENT_COUNT = 0
	ISDBT_LAYERA_TIME_INTERLEAVING = 0
	ISDBT_LAYERB_FEC = AUTO
	ISDBT_LAYERB_MODULATION = QAM/AUTO
	ISDBT_LAYERB_SEGMENT_COUNT = 0
	ISDBT_LAYERB_TIME_INTERLEAVING = 0
	ISDBT_LAYERC_FEC = AUTO
	ISDBT_LAYERC_MODULATION = QAM/AUTO
	ISDBT_LAYERC_SEGMENT_COUNT = 0
	ISDBT_LAYERC_TIME_INTERLEAVING = 0

# Physical channel 18 (virtual 4.1)
[Record GoiÃ¡s]
	DELIVERY_SYSTEM = ISDBT
	BANDWIDTH_HZ = 6000000
	FREQUENCY = 497142857
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	ISDBT_LAYER_ENABLED = 7
	ISDBT_SOUND_BROADCASTING = 0
	ISDBT_SB_SUBCHANNEL_ID = 0
	ISDBT_SB_SEGMENT_IDX = 0
	ISDBT_SB_SEGMENT_COUNT = 0
	ISDBT_LAYERA_FEC = AUTO
	ISDBT_LAYERA_MODULATION = QAM/AUTO
	ISDBT_LAYERA_SEGMENT_COUNT = 0
	ISDBT_LAYERA_TIME_INTERLEAVING = 0
	ISDBT_LAYERB_FEC = AUTO
	ISDBT_LAYERB_MODULATION = QAM/AUTO
	ISDBT_LAYERB_SEGMENT_COUNT = 0
	ISDBT_LAYERB_TIME_INTERLEAVING = 0
	ISDBT_LAYERC_FEC = AUTO
	ISDBT_LAYERC_MODULATION = QAM/AUTO
	ISDBT_LAYERC_SEGMENT_COUNT = 0
	ISDBT_LAYERC_TIME_INTERLEAVING = 0

# Physical channel 20 (virtual 9.1)
[TV Serra Dourada]
	DELIVERY_SYSTEM = ISDBT
	BANDWIDTH_HZ = 6000000
	FREQUENCY = 509142857
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	ISDBT_LAYER_ENABLED = 7
	ISDBT_SOUND_BROADCASTING = 0
	ISDBT_SB_SUBCHANNEL_ID = 0
	ISDBT_SB_SEGMENT_IDX = 0
	ISDBT_SB_SEGMENT_COUNT = 0
	ISDBT_LAYERA_FEC = AUTO
	ISDBT_LAYERA_MODULATION = QAM/AUTO
	ISDBT_LAYERA_SEGMENT_COUNT = 0
	ISDBT_LAYERA_TIME_INTERLEAVING = 0
	ISDBT_LAYERB_FEC = AUTO
	ISDBT_LAYERB_MODULATION = QAM/AUTO
	ISDBT_LAYERB_SEGMENT_COUNT = 0
	ISDBT_LAYERB_TIME_INTERLEAVING = 0
	ISDBT_LAYERC_FEC = AUTO
	ISDBT_LAYERC_MODULATION = QAM/AUTO
	ISDBT_LAYERC_SEGMENT_COUNT = 0
	ISDBT_LAYERC_TIME_INTERLEAVING = 0

# Physical channel 22 (virtual 24.1)
[PUC TV GoiÃ¡s]
	DELIVERY_SYSTEM = ISDBT
	BANDWIDTH_HZ = 6000000
	FREQUENCY = 521142857
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	ISDBT_LAYER_ENABLED = 7
	ISDBT_SOUND_BROADCASTING = 0
	ISDBT_SB_SUBCHANNEL_ID = 0
	ISDBT_SB_SEGMENT_IDX = 0
	ISDBT_SB_SEGMENT_COUNT = 0
	ISDBT_LAYERA_FEC = AUTO
	ISDBT_LAYERA_MODULATION = QAM/AUTO
	ISDBT_LAYERA_SEGMENT_COUNT = 0
	ISDBT_LAYERA_TIME_INTERLEAVING = 0
	ISDBT_LAYERB_FEC = AUTO
	ISDBT_LAYERB_MODULATION = QAM/AUTO
	ISDBT_LAYERB_SEGMENT_COUNT = 0
	ISDBT_LAYERB_TIME_INTERLEAVING = 0
	ISDBT_LAYERC_FEC = AUTO
	ISDBT_LAYERC_MODULATION = QAM/AUTO
	ISDBT_LAYERC_SEGMENT_COUNT = 0
	ISDBT_LAYERC_TIME_INTERLEAVING = 0

# Physical channel 29 (virtual 29.1)
[TV Pai Eterno]
	DELIVERY_SYSTEM = ISDBT
	BANDWIDTH_HZ = 6000000
	FREQUENCY = 563142857
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	ISDBT_LAYER_ENABLED = 7
	ISDBT_SOUND_BROADCASTING = 0
	ISDBT_SB_SUBCHANNEL_ID = 0
	ISDBT_SB_SEGMENT_IDX = 0
	ISDBT_SB_SEGMENT_COUNT = 0
	ISDBT_LAYERA_FEC = AUTO
	ISDBT_LAYERA_MODULATION = QAM/AUTO
	ISDBT_LAYERA_SEGMENT_COUNT = 0
	ISDBT_LAYERA_TIME_INTERLEAVING = 0
	ISDBT_LAYERB_FEC = AUTO
	ISDBT_LAYERB_MODULATION = QAM/AUTO
	ISDBT_LAYERB_SEGMENT_COUNT = 0
	ISDBT_LAYERB_TIME_INTERLEAVING = 0
	ISDBT_LAYERC_FEC = AUTO
	ISDBT_LAYERC_MODULATION = QAM/AUTO
	ISDBT_LAYERC_SEGMENT_COUNT = 0
	ISDBT_LAYERC_TIME_INTERLEAVING = 0

# Physical channel 30 (virtual 11.1)
[TV GoiÃ¢nia]
	DELIVERY_SYSTEM = ISDBT
	BANDWIDTH_HZ = 6000000
	FREQUENCY = 569142857
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	ISDBT_LAYER_ENABLED = 7
	ISDBT_SOUND_BROADCASTING = 0
	ISDBT_SB_SUBCHANNEL_ID = 0
	ISDBT_SB_SEGMENT_IDX = 0
	ISDBT_SB_SEGMENT_COUNT = 0
	ISDBT_LAYERA_FEC = AUTO
	ISDBT_LAYERA_MODULATION = QAM/AUTO
	ISDBT_LAYERA_SEGMENT_COUNT = 0
	ISDBT_LAYERA_TIME_INTERLEAVING = 0
	ISDBT_LAYERB_FEC = AUTO
	ISDBT_LAYERB_MODULATION = QAM/AUTO
	ISDBT_LAYERB_SEGMENT_COUNT = 0
	ISDBT_LAYERB_TIME_INTERLEAVING = 0
	ISDBT_LAYERC_FEC = AUTO
	ISDBT_LAYERC_MODULATION = QAM/AUTO
	ISDBT_LAYERC_SEGMENT_COUNT = 0
	ISDBT_LAYERC_TIME_INTERLEAVING = 0

# Physical channel 31 (virtual 13.1)
[TV Brasil Central]
	DELIVERY_SYSTEM = ISDBT
	BANDWIDTH_HZ = 6000000
	FREQUENCY = 575142857
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	ISDBT_LAYER_ENABLED = 7
	ISDBT_SOUND_BROADCASTING = 0
	ISDBT_SB_SUBCHANNEL_ID = 0
	ISDBT_SB_SEGMENT_IDX = 0
	ISDBT_SB_SEGMENT_COUNT = 0
	ISDBT_LAYERA_FEC = AUTO
	ISDBT_LAYERA_MODULATION = QAM/AUTO
	ISDBT_LAYERA_SEGMENT_COUNT = 0
	ISDBT_LAYERA_TIME_INTERLEAVING = 0
	ISDBT_LAYERB_FEC = AUTO
	ISDBT_LAYERB_MODULATION = QAM/AUTO
	ISDBT_LAYERB_SEGMENT_COUNT = 0
	ISDBT_LAYERB_TIME_INTERLEAVING = 0
	ISDBT_LAYERC_FEC = AUTO
	ISDBT_LAYERC_MODULATION = QAM/AUTO
	ISDBT_LAYERC_SEGMENT_COUNT = 0
	ISDBT_LAYERC_TIME_INTERLEAVING = 0

# Physical channel 34 (virtual 2.1)
[TV Anhanguera GoiÃ¢nia]
	DELIVERY_SYSTEM = ISDBT
	BANDWIDTH_HZ = 6000000
	FREQUENCY = 593142857
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	ISDBT_LAYER_ENABLED = 7
	ISDBT_SOUND_BROADCASTING = 0
	ISDBT_SB_SUBCHANNEL_ID = 0
	ISDBT_SB_SEGMENT_IDX = 0
	ISDBT_SB_SEGMENT_COUNT = 0
	ISDBT_LAYERA_FEC = AUTO
	ISDBT_LAYERA_MODULATION = QAM/AUTO
	ISDBT_LAYERA_SEGMENT_COUNT = 0
	ISDBT_LAYERA_TIME_INTERLEAVING = 0
	ISDBT_LAYERB_FEC = AUTO
	ISDBT_LAYERB_MODULATION = QAM/AUTO
	ISDBT_LAYERB_SEGMENT_COUNT = 0
	ISDBT_LAYERB_TIME_INTERLEAVING = 0
	ISDBT_LAYERC_FEC = AUTO
	ISDBT_LAYERC_MODULATION = QAM/AUTO
	ISDBT_LAYERC_SEGMENT_COUNT = 0
	ISDBT_LAYERC_TIME_INTERLEAVING = 0

# Physical channel 47 (virtual 5.1)
[Fonte TV]
	DELIVERY_SYSTEM = ISDBT
	BANDWIDTH_HZ = 6000000
	FREQUENCY = 671142857
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	ISDBT_LAYER_ENABLED = 7
	ISDBT_SOUND_BROADCASTING = 0
	ISDBT_SB_SUBCHANNEL_ID = 0
	ISDBT_SB_SEGMENT_IDX = 0
	ISDBT_SB_SEGMENT_COUNT = 0
	ISDBT_LAYERA_FEC = AUTO
	ISDBT_LAYERA_MODULATION = QAM/AUTO
	ISDBT_LAYERA_SEGMENT_COUNT = 0
	ISDBT_LAYERA_TIME_INTERLEAVING = 0
	ISDBT_LAYERB_FEC = AUTO
	ISDBT_LAYERB_MODULATION = QAM/AUTO
	ISDBT_LAYERB_SEGMENT_COUNT = 0
	ISDBT_LAYERB_TIME_INTERLEAVING = 0
	ISDBT_LAYERC_FEC = AUTO
	ISDBT_LAYERC_MODULATION = QAM/AUTO
	ISDBT_LAYERC_SEGMENT_COUNT = 0
	ISDBT_LAYERC_TIME_INTERLEAVING = 0

# Physical channel 49 (virtual 49.1)
[Rede SÃ©culo 21 Educa, Rede SÃ©culo 21]
	DELIVERY_SYSTEM = ISDBT
	BANDWIDTH_HZ = 6000000
	FREQUENCY = 683142857
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	ISDBT_LAYER_ENABLED = 7
	ISDBT_SOUND_BROADCASTING = 0
	ISDBT_SB_SUBCHANNEL_ID = 0
	ISDBT_SB_SEGMENT_IDX = 0
	ISDBT_SB_SEGMENT_COUNT = 0
	ISDBT_LAYERA_FEC = AUTO
	ISDBT_LAYERA_MODULATION = QAM/AUTO
	ISDBT_LAYERA_SEGMENT_COUNT = 0
	ISDBT_LAYERA_TIME_INTERLEAVING = 0
	ISDBT_LAYERB_FEC = AUTO
	ISDBT_LAYERB_MODULATION = QAM/AUTO
	ISDBT_LAYERB_SEGMENT_COUNT = 0
	ISDBT_LAYERB_TIME_INTERLEAVING = 0
	ISDBT_LAYERC_FEC = AUTO
	ISDBT_LAYERC_MODULATION = QAM/AUTO
	ISDBT_LAYERC_SEGMENT_COUNT = 0
	ISDBT_LAYERC_TIME_INTERLEAVING = 0

