# DVB-T Cadiz (Andalusia)                      by xiterrex  Aug 2014
# Info obtained from Spanish Government (Ministerio de Industria) at URL:
# <http://www.minetur.gob.es/telecomunicaciones/infraestructuras/paginas/tdt_ict.aspx>
[C21 # MPE2]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 474000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[C23 # RGE1]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 490000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[C24 # RGE1]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 498000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

# 498000000 8MHz 2/3 NONE QAM64 8k 1/4 NONE    # C24 # TL02CA Arcos
[C27 # RGE2]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 522000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

# 522000000 8MHz 2/3 NONE QAM64 8k 1/4 NONE    # C27 # TL06CA Olvera
[C28 # TL01CA Algeciras]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 530000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[C30 # TL05CA Jerez]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 546000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[C33 # RGE2 (Main)]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 570000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[C38 # MPE3]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 610000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[C41 # MPE2]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 634000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[C43 # TL08CA Medina]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 650000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[C44 # MPE1]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 658000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[C46 # AND]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 674000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[C49 # MPE3 (Main)]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 698000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[C50 # TL07CA Ubrique]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 706000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[C52 # RGE2]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 722000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

# 722000000 8MHz 2/3 NONE QAM64 8k 1/4 NONE    # C52 # TL04CA Chiclana
[C53 # MPE1 (Main)]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 730000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[C54 # TL03CA Cadiz]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 738000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[C55 # MPE2 (Main)]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 746000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[C57 # RGE1 (Main)]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 762000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[C59 # AND (Main)]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 778000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[C64 # RGE1]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 818000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[C67 # MD67]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 842000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[C68 # MD68]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 850000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[C69 # MD69]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 858000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

