# Funciona correctamente en Santa Cruz de Tenerife (25-09-2010)
# 
# Revisada y corregida por el Grupo de Usuarios de Linux de Canarias
# http://www.gulic.org
#
[C23]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 490000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[C24]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 498000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[C26]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 514000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[C29]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 538000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[C45]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 666000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[C56]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 754000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[C59]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 778000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[C60]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 786000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[C66]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 834000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[C67]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 842000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[C68]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 850000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[C69]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 858000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

