# Channel table for Express AT2 at 140.0°E
# Source: http://www.lyngsat.com/Express-AT2.html

[various]
	DELIVERY_SYSTEM = DVBS2
	FREQUENCY = 12188000
	POLARIZATION = LEFT
	SYMBOL_RATE = 27500000
	MODULATION = PSK/8
	INNER_FEC = AUTO
	INVERSION = AUTO

[NTV Plus Dalniy Vostok]
	DELIVERY_SYSTEM = DVBS2
	FREQUENCY = 12245000
	POLARIZATION = RIGHT
	SYMBOL_RATE = 27500000
	MODULATION = PSK/8
	INNER_FEC = AUTO
	INVERSION = AUTO

[NTV Plus Dalniy Vostok]
	DELIVERY_SYSTEM = DVBS2
	FREQUENCY = 12303000
	POLARIZATION = LEFT
	SYMBOL_RATE = 27500000
	MODULATION = PSK/8
	INNER_FEC = AUTO
	INVERSION = AUTO

[NTV Plus Dalniy Vostok]
	DELIVERY_SYSTEM = DVBS2
	FREQUENCY = 12322000
	POLARIZATION = RIGHT
	SYMBOL_RATE = 27500000
	MODULATION = PSK/8
	INNER_FEC = AUTO
	INVERSION = AUTO

[NTV Plus Dalniy Vostok]
	DELIVERY_SYSTEM = DVBS2
	FREQUENCY = 12380000
	POLARIZATION = LEFT
	SYMBOL_RATE = 27500000
	MODULATION = PSK/8
	INNER_FEC = AUTO
	INVERSION = AUTO

[NTV Plus Dalniy Vostok]
	DELIVERY_SYSTEM = DVBS2
	FREQUENCY = 12399000
	POLARIZATION = RIGHT
	SYMBOL_RATE = 27500000
	MODULATION = PSK/8
	INNER_FEC = AUTO
	INVERSION = AUTO

[NTV Plus Dalniy Vostok]
	DELIVERY_SYSTEM = DVBS2
	FREQUENCY = 12476000
	POLARIZATION = RIGHT
	SYMBOL_RATE = 27500000
	MODULATION = PSK/8
	INNER_FEC = AUTO
	INVERSION = AUTO

